**Name of work place:**        **Assessment conducted by:**

**Work place address:**       **Date of assessment:**

**Work area(s):**       **PPE Selected By:**

**Job/Task(s):**       **Effective Date:**

|  |  |  |
| --- | --- | --- |
| EYES/FACE |  [ ]  Negligible Hazard |  **Can hazard be eliminated without the use of PPE? Yes [ ]  No** [ ]  |
| Work-related exposure to:[ ]  airborne dust[ ]  flying particles[ ]  hazardous liquids/chemicals[ ]  intense light[ ]  blood splashes[ ]  other:       | PPE required to manage hazard:[ ]  Safety glasses [ ]  Safety goggles[ ]  Face Shield [ ]  Shading/Filter (#     ) [ ]  Welding shield[ ]  Other:       | Comments:      |
| HEAD |  [ ]  Negligible Hazard |  **Can hazard be eliminated without the use of PPE? Yes [ ]  No** [ ]  |
| Work-related exposure to:[ ]  beams[ ]  pipes[ ]  falling objects[ ]  exposed electrical wiring or components[ ]  machine parts [ ]  other:       | PPE required to manage hazard:[ ]  Protective Helmet[ ]  Type A (low voltage)[ ]  Type B (high voltage)[ ]  Type C[ ]  Hair net or soft cap[ ]  Other:       | Comments:      |
| HANDS/ARMS |  [ ]  Negligible Hazard |  **Can hazard be eliminated without the use of PPE? Yes [ ]  No** [ ]  |
| Work-related exposure to:[ ]  hazardous liquids/chemicals[ ]  scrapes, bruise, or cut [ ]  injuries from tools [ ]  extreme heat/cold[ ]  blood (OPIM)[ ]  other:       | PPE required to manage hazard:[ ]  Gloves[ ]  Chemical resistance [ ]  Liquid/leak resistance[ ]  Temperature resistance [ ]  Cut resistance[ ]  Gauntlet or long necked [ ]  Work Gloves[ ]  Chemical Protective sleeves[ ]  Long sleeves[ ]  Other:       | Comments: |
| FEET/LEGS |  [ ]  Negligible Hazard |  **Can hazard be eliminated without the use of PPE? Yes [ ]  No** [ ]  |
| Work-related exposure to:[ ]  hazardous liquids/chemicals[ ]  heavy falling/rolling objects[ ]  heavy equipment [ ]  exposed electrical wiring or components[ ]  slippery surfaces[ ]  explosive atmospheres[ ]  tools[ ]  other:       | PPE required to manage hazard:[ ]  closed shoes (e.g. no opened toes or sandals)[ ]  long pants[ ]  Safety shoes or boots[ ]  Toe protection [ ]  Metatarsal protection[ ]  Electrical protection [ ]  Heat/cold protection[ ]  Anti-slip soles [ ]  Chemical resistance[ ]  Leggings or chaps[ ]  Foot-Leg guards[ ]  Other:       | Comments:  |
| BODY/SKIN |  [ ]  Negligible Hazard |  **Can hazard be eliminated without the use of PPE? Yes [ ]  No** [ ]  |
| Work-related exposure to:[ ]  hazardous liquids/chemicals[ ]  sharp or rough edges [ ]  extreme heat/cold[ ]  other:       | PPE required to manage hazard:[ ]  Lab Coat [ ]  Raingear[ ]  Coveralls, Body suit [ ]  Apron[ ]  Welding leathers [ ]  Abrasion/cut [ ]  Other:       resistance | Comments:      |
| BODY/WHOLE |  [ ]  Negligible Hazard |  **Can hazard be eliminated without the use of PPE? Yes [ ]  No** [ ]  |
| Work-related exposure to:[ ]  working from heights of 4 feet or more[ ]  working near water[ ]  other:       | PPE required to manage hazard:[ ]  Fall Arrest/Restraint: Type:      [ ]  PFD: Type:      [ ]  Other:       | Comments:      |
| LUNGS/EARS |  [ ]  Negligible Hazard |  **Can hazard be eliminated without the use of PPE? Yes [ ]  No** [ ]  |
| Work-related exposure to:[ ]  irritating dust or particulate[ ]  irritating or toxic gas/vapor[ ]  loud work environment[ ]  noisy machines/tools[ ]  other:       | PPE required to manage hazard:[ ]  Respirator (Cartridge type:      )[ ]  Particulate Mask[ ]  Hearing Protection | Comments:      |