**Name of work place:**        **Assessment conducted by:**

**Work place address:**       **Date of assessment:**

**Work area(s):**       **PPE Selected By:**

**Job/Task(s):**       **Effective Date:**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| EYES/FACE | Negligible Hazard | | **Can hazard be eliminated without the use of PPE? Yes  No** | |
| Work-related exposure to:  airborne dust  flying particles  hazardous liquids/chemicals  intense light  blood splashes  other: | | PPE required to manage hazard:  Safety glasses  Safety goggles  Face Shield  Shading/Filter (#     )  Welding shield  Other: | | Comments: |
| HEAD | Negligible Hazard | | **Can hazard be eliminated without the use of PPE? Yes  No** | |
| Work-related exposure to:  beams  pipes  falling objects  exposed electrical wiring or components  machine parts  other: | | PPE required to manage hazard:  Protective Helmet  Type A (low voltage)  Type B (high voltage)  Type C  Hair net or soft cap  Other: | | Comments: |
| HANDS/ARMS | Negligible Hazard | | **Can hazard be eliminated without the use of PPE? Yes  No** | |
| Work-related exposure to:  hazardous liquids/chemicals  scrapes, bruise, or cut  injuries from tools  extreme heat/cold  blood (OPIM)  other: | | PPE required to manage hazard:  Gloves  Chemical resistance  Liquid/leak resistance  Temperature resistance  Cut resistance  Gauntlet or long necked  Work Gloves  Chemical Protective sleeves  Long sleeves  Other: | | Comments: |
| FEET/LEGS | Negligible Hazard | | **Can hazard be eliminated without the use of PPE? Yes  No** | |
| Work-related exposure to:  hazardous liquids/chemicals  heavy falling/rolling objects  heavy equipment  exposed electrical wiring or components  slippery surfaces  explosive atmospheres  tools  other: | | PPE required to manage hazard:  closed shoes (e.g. no opened toes or sandals)  long pants  Safety shoes or boots  Toe protection  Metatarsal protection  Electrical protection  Heat/cold protection  Anti-slip soles  Chemical resistance  Leggings or chaps  Foot-Leg guards  Other: | | Comments: |
| BODY/SKIN | Negligible Hazard | | **Can hazard be eliminated without the use of PPE? Yes  No** | |
| Work-related exposure to:  hazardous liquids/chemicals  sharp or rough edges  extreme heat/cold  other: | | PPE required to manage hazard:  Lab Coat  Raingear  Coveralls, Body suit  Apron  Welding leathers  Abrasion/cut  Other:       resistance | | Comments: |
| BODY/WHOLE | Negligible Hazard | | **Can hazard be eliminated without the use of PPE? Yes  No** | |
| Work-related exposure to:  working from heights of 4 feet or more  working near water  other: | | PPE required to manage hazard:  Fall Arrest/Restraint: Type:  PFD: Type:  Other: | | Comments: |
| LUNGS/EARS | Negligible Hazard | | **Can hazard be eliminated without the use of PPE? Yes  No** | |
| Work-related exposure to:  irritating dust or particulate  irritating or toxic gas/vapor  loud work environment  noisy machines/tools  other: | | PPE required to manage hazard:  Respirator (Cartridge type:      )  Particulate Mask  Hearing Protection | | Comments: |